Ultrasonic Sensor:

GND: Black

Vcc: Red

Echo:Green

Trigger:Yellow

Mtor driver

Inner edge pin